# Network Benchmarks

## GCC Cortex-M4F Size Benchmarks

> Note, these benchmarks are under development! This initial report simply describes memory footprint data for some network examples in the SimpleLink SDKs. Those examples are not optimized, so memory usage reported here reflects higher than minimal memory usage. We’re working on providing more data in future releases.

Board: MSP432E4 LaunchPad

Tool Chain Version: gcc-arm-none-eabi-7-2017-q4-major

RTOS Version: SYS/BIOS 6.76.00.08

## Network Applications

> Note, all sizes are in 8-bit bytes

Application Name | Code | Initialized Data | C-initialization | Total Flash | ISR/C Stack | Task Stacks | Heaps | BSS | Total RAM
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
basic | 111566 | 0 | 0 | 111566 | 1536 | 0 | 20480 | 24456 | 46472
httpget | 119366 | 0 | 0 | 119366 | 1024 | 0 | 131072 | 45512 | 177608
httpserver | 408152 | 0 | 0 | 408152 | 1024 | 0 | 131072 | 51900 | 183996
httpsget | 408124 | 0 | 0 | 408124 | 1024 | 0 | 131072 | 49124 | 181220
mqttclient | 413614 | 0 | 0 | 413614 | 1024 | 0 | 131072 | 52256 | 184352
mqttclientserver | 426746 | 0 | 0 | 426746 | 1024 | 0 | 131072 | 57320 | 189416
tcpecho | 110814 | 0 | 0 | 110814 | 1024 | 0 | 131072 | 45484 | 177580
tcpechotls | 401528 | 0 | 0 | 401528 | 1024 | 0 | 131072 | 52772 | 184868
udpecho | 110770 | 0 | 0 | 110770 | 1024 | 0 | 131072 | 45484 | 177580
udpechoipv6 | 150830 | 0 | 0 | 150830 | 1024 | 0 | 131072 | 46264 | 178360