# Network Benchmarks

## IAR Cortex-M4F Size Benchmarks

> Note, these benchmarks are under development! This initial report simply describes memory footprint data for some network examples in the SimpleLink SDKs. Those examples are not optimized, so memory usage reported here reflects higher than minimal memory usage. We’re working on providing more data in future releases.

Board: MSP432E4 LaunchPad

Tool Chain Version: 8.32.2

RTOS Version: SYS/BIOS 6.76.00.08

## Network Applications

> Note, all sizes are in 8-bit bytes

Application Name | Code | Initialized Data | C-initialization | Total Flash | ISR/C Stack | Task Stacks | Heaps | BSS | Total RAM
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
basic | 103866 | 0 | 0 | 103866 | 0 | 0 | 20480 | 4873 | 25353
httpget | 114462 | 0 | 0 | 114462 | 0 | 0 | 131072 | 44372 | 175444
httpserver | 327645 | 0 | 0 | 327645 | 0 | 0 | 131072 | 50168 | 181240
httpsget | 327166 | 0 | 0 | 327166 | 0 | 0 | 131072 | 47008 | 178080
mqttclient | 332441 | 0 | 0 | 332441 | 0 | 0 | 131072 | 50266 | 181338
mqttclientserver | 347067 | 0 | 0 | 347067 | 0 | 0 | 131072 | 54887 | 185959
tcpecho | 104309 | 0 | 0 | 104309 | 0 | 0 | 131072 | 44086 | 175158
tcpechotls | 321446 | 0 | 0 | 321446 | 0 | 0 | 131072 | 50078 | 181150
udpecho | 104086 | 0 | 0 | 104086 | 0 | 0 | 131072 | 44082 | 175154
udpechoipv6 | 143897 | 0 | 0 | 143897 | 0 | 0 | 131072 | 44970 | 176042