# Network Benchmarks

## IAR Cortex-M4F Size Benchmarks

> Note, these benchmarks are under development! This initial report simply describes memory footprint data for some network examples in the SimpleLink SDKs. Those examples are not optimized, so memory usage reported here reflects higher than minimal memory usage. We’re working on providing more data in future releases.

Board: MSP432E4 LaunchPad

Tool Chain Version: 8.32.2

RTOS Version: FreeRTOS 10.1.1

## Network Applications

> Note, all sizes are in 8-bit bytes

Application Name | Code | Initialized Data | C-initialization | Total Flash | ISR/C Stack | Task Stacks | Heaps | BSS | Total RAM
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
basic | 85537 | 0 | 0 | 85537 | 0 | 0 | 20480 | 29783 | 50263
httpget | 110544 | 0 | 0 | 110544 | 0 | 0 | 131072 | 48984 | 180056
httpserver | 322357 | 0 | 0 | 322357 | 0 | 0 | 131072 | 54156 | 185228
httpsget | 322848 | 0 | 0 | 322848 | 0 | 0 | 131072 | 50988 | 182060
mqttclient | 327283 | 0 | 0 | 327283 | 0 | 0 | 131072 | 54258 | 185330
mqttclientserver | 341897 | 0 | 0 | 341897 | 0 | 0 | 131072 | 58879 | 189951
tcpecho | 100393 | 0 | 0 | 100393 | 0 | 0 | 131072 | 47962 | 179034
tcpechotls | 317130 | 0 | 0 | 317130 | 0 | 0 | 131072 | 54058 | 185130
udpecho | 100170 | 0 | 0 | 100170 | 0 | 0 | 131072 | 47958 | 179030
udpechoipv6 | 139977 | 0 | 0 | 139977 | 0 | 0 | 131072 | 49494 | 180566