# NDK 3.61.01.01 Release Notes

## Table of Contents

## Introduction

The Network Developer’s Kit (NDK) is a platform for development and demonstration of network enabled applications on TI embedded processors.

Depending on your platform and distribution, you may need to separately obtain an appropriate NDK Support Package (NSP).

## Documentation

The following documentation is provided with this release.

- Documentation Overview

## What’s New

### 3.61.01.01

#### Defects

The following Defects were resolved

ID | Summary
--- | ---
None | None

#### Enhancements

The following Enhancements were resolved

ID | Summary
--- | ---
NDK-277 | Add NIMU driver for F2838X

## Upgrade and Compatibility Information

NDK 3.61 is compatible with 3.60.

If updating from a previous version of NDK, see the changelog for potential upgrade and compatibility information.

A few notable feature deprecation alerts:

- The NDK’s HTTP/1.0 Server will be removed in a future release, likely in late 2019. The Network Services Component is now providing a much more fully featured HTTP/1.1 Server, which is recommended for new development. Related scripts/tools (e.g. ti/ndk/tools/binsrc) are also deprecated and are planned for removal.
- The host executables provided in ti/ndk/winapps are also deprecated. These scripts do not provide significant value, and are also planned for removal in a future release, likely in late 2019.

## Host Support

- Windows
- Linux
- Mac

## Dependencies

This release requires the following software components and tools versions to successfully function:

- SYS/BIOS 6.76.00.08
- Network Services 2.60.00.07

## Toolchain Support

The NDK supports building libraries for the following ISA/toolchain combinations, your SDK may provide a subset of these libraries:

ISA | TI/CCS | IAR | GCC
--- | --- | --- | ---
C674x | 8.3.2 | N/A | N/A
C66 | 8.3.2 | N/A | N/A
Arm9 | 18.12.1.LTS | N/A | N/A
A8F | N/A | N/A | gcc-arm-none-eabi-7-2017-q4-major
A9F | N/A | N/A | gcc-arm-none-eabi-7-2017-q4-major
A15F | N/A | N/A | gcc-arm-none-eabi-7-2017-q4-major
A53F | N/A | N/A | gcc-linaro-7.2.1-2017.11-x86_64_aarch64-elf
M4 | 18.12.1.LTS | N/A | N/A
M4F | 18.12.1.LTS | 8.32.2 | gcc-arm-none-eabi-7-2017-q4-major
R5F | 18.12.1.LTS | N/A | N/A

## Device Support

Please refer to the SDK Release Notes for device support.

## Known Issues

- Stack shut down and or reboot is not supported on F2838X
  - Code to handle shut down and/or restarting of the EMAC DMA engine is not currently implemented and will be added in a future release.
  - The following Jira has been filed to track this issue:
    - NDK-405: Update F2838X NIMU driver to support stack reboot/shutdown
- A crash was witnessed during system test which appears to be a memory corruption issue. It’s unclear whether this is an issue in the NDK/driver or test case.
  - The cause of this issue is still under investigation.
  - The following Jira has been filed to track this issue:
    - NDK-406: Crash due to possible memory corruption seen on F2838X

## Versioning

All releases have 4 segment versions (M.mm.pp.bb). This includes GA and pre-releases (engineering, alpha/EA, beta, etc.). Pre-releases are denoted with a suffix (e.g. 3.40.00.00_eng).

This product’s version follows a version format, M.mm.pp.bb, where M is a single digit Major number, mm is 2 digit minor number, pp is a 2 digit patch number, and bb is an unrestricted set of digits used as an incrementing build counter.

Subsequent releases of patch upgrades will be identified by the patch number. Typically, these patches only include critical bug fixes.

## Technical Support

- TI E2E Community

Last updated: 2019-05-28